;
;               Omicron SPM Control.
;           Parameter file for SPM data.
;
; Original experiment: 'STM_Spectroscopy', result creator: MATRIX V4.3.2-_v1843-tag-release-MatrixKit_4.3.2-206476
; Original result data file specification: X:\Raw Data\2022\2022.06.06.LHe_Wtip_Au111_78a_Tsublim_80C_4min+8min_220C_10min\20220606-STM_Spectroscopy-Au111--334_1.I_mtrx
; Original run/scan cycle identification: 334-1
; Generated by Vernissage SCALA PRO Formatter version V1.9 (Demo)
;

Format                          : 1

Version                         : 5.0
System                          : SCALA

;
; User Information.
;

Date                            : 07.06.2022 19:16
User                            : Administrator
Comment                         : 

;
; Scanner Description.
;

Name                            : -
VGAP Contact                    : -

;
; Scan Area Description.
;

Field X Size in nm              :  3.0000     ;[nm]
Field Y Size in nm              :  3.0000     ;[nm]
Image Size in X                 : 256
Image Size in Y                 : 256
Increment X                     : 0.011719      ;[nm]
Increment Y                     : 0.011719      ;[nm]
Scan Angle                      : 347.000000      ;[Degree]
X Offset                        : 160.424069      ;[nm]
Y Offset                        : -156.666388      ;[nm]

;
; Topographic Channels.
;

; Result data file: X:\Raw Data\2022\2022.06.06.LHe_Wtip_Au111_78a_Tsublim_80C_4min+8min_220C_10min\20220606-STM_Spectroscopy-Au111--334_1.I_mtrx

Topographic Channel             : I   ;Channel
                                  Forward
                                  -32768   ;Minimum raw value
                                  32767   ;Maximum raw value
                                   -3.297   ;Minimum value in physical unit
                                    3.297   ;Maximum value in physical unit
                                  0.000100617   ;Resolution
                                  nA   ;Physical unit
                                  m1_ori.tf0   ;Filename
                                  I   ;Display name

; Result data file: X:\Raw Data\2022\2022.06.06.LHe_Wtip_Au111_78a_Tsublim_80C_4min+8min_220C_10min\20220606-STM_Spectroscopy-Au111--334_1.I_mtrx

Topographic Channel             : I   ;Channel
                                  Backward
                                  -32768   ;Minimum raw value
                                  32767   ;Maximum raw value
                                   -3.297   ;Minimum value in physical unit
                                    3.297   ;Maximum value in physical unit
                                  0.000100617   ;Resolution
                                  nA   ;Physical unit
                                  m1_ori.tb0   ;Filename
                                  I   ;Display name

;
; Measurement parameters.
;

SPM Method                      : STM
Dual mode                       : Off
Gap Voltage                     : 0.00500     ;[V]
Feedback Set                    : 0.05     ;[nA]
Loop Gain                       : 3.00000     ;[%]
X Resolution                    : 0     ;Currently not used.
Y Resolution                    : 0     ;Currently not used.
Measured Gap Voltage            : 0.00500     ;[V] (not really supported)
Measured Current Setpoint       : 0.05     ;[nA] (not really supported)
Measured Current                : 0     ;[nA] (not supported)
Scan Speed                      : 11.719     ;[nm/s]
X Drift                         : 0.000000     ;[nm/s]
Y Drift                         : 0.000000     ;[nm/s]
Scan Mode                       : Frame
Scan Direction                  : UP
Topography Time per Point       : 0.001000
Spectroscopy Grid Value in X    : 10
Spectroscopy Grid Value in Y    : 10
Spectroscopy Points in X        : 26
Spectroscopy Lines in Y         : 26

;
; Z Control Parameters.
;

Z Speed                         : 0.00     ;[nm/s]
Z Output Gain                   : 1.000000
Automatic Z zero                : On
Z Input Gain                    : 1.000

;
; AFM Description.
;

AFM exists                      : 0
Amplitude                       : 0.000000
Delta f sign                    : +1
Oscillator available?           : No
Calibration FN                  : 10.000000
Calibration FL                  : 10.000000
I Total                         : 0.0000000000
